Jump to main content

# Unisphere policy name - Alert ID mapping

The following table presents an overview of Unisphere policy names and their corresponding Solutions Enabler Alert/Event IDs. For details on the events, use the hyperlinks.

| NOTE: Hotspare events are not supported for arrays running PowerMaxOS 10 (6079) and higher.

Table 1. Unisphere policy name - Alert ID mapping
Unisphere policy name | Alert/Event ID | Solutions Enabler event definition
--- | --- | ---
Hot spare Invoked | 1054 | SYMAPI_AEVENT2_UID_MOD_DISKDRV_SPARE_INVK
1060 | SYMAPI_AEVENT2_UID_MOD_RDF_HOTSPARE_INVK
1210 | SYMAPI_AEVENT2_UID_ALERT_HOTSPARE_CHANGE
Port Link Status | 1063 | SYMAPI_AEVENT2_UID_MOD_FCPORT_FAIL
Environmental Alert | 1067 | SYMAPI_AEVENT2_UID_MOD_TEMP_OUT_OF_LIMIT
1150 | SYMAPI_AEVENT2_UID_MOD_LCC_A_TEMP_HIGH
1151 | SYMAPI_AEVENT2_UID_MOD_LCC_B_TEMP_HIGH
SRDF/A Session entering Transmit Idle state | 1138 | SYMAPI_AEVENT2_UID_MOD_SRDFA_SE_TRANS_IDLE
SRDF/A Session recovered from a Transmit Idle state | 1139 | SYMAPI_AEVENT2_UID_MOD_SRDFA_SR_TRANS_IDLE
SRDF/A Session dropped, transit idle state timeout | 1140 | SYMAPI_AEVENT2_UID_MOD_SRDFA_TO_TRANS_IDLE
SRDF/A No Cycle Switch Alert | 1159 | SYMAPI_AEVENT2_UID_ALERT_SRDFA_NO_CYCLE_SWITCH
SRDF Job Flow Control Change | 1160 | SYMAPI_AEVENT2_UID_ALERT_SRDF_JFC_STATE_CHANGE
External disk group fully allocated | 1162 | SYMAPI_AEVENT2_UID_ALERT_EDISK_FULL
Device Status | 1200 | SYMAPI_AEVENT2_UID_ALERT_DEV_STATUS
Director Status | 1202 | SYMAPI_AEVENT2_UID_ALERT_DIRECTOR_STATUS
Port Status | 1203 | SYMAPI_AEVENT2_UID_ALERT_PORT_STATUS
Disk status | 1204 | SYMAPI_AEVENT2_UID_ALERT_DISK_STATUS
Thin Device Allocation | 1212 | SYMAPI_AEVENT2_UID_THRESH_TDEV_ALLOCATED
Thin Device Usage | 1213 | SYMAPI_AEVENT2_UID_THRESH_TDEV_USED
Deferred Service Threshold Alert | 1217 | SYMAPI_AEVENT2_UID_ALERT_DFR_SVC_STATE
Array Component Events | 1244 | SYMAPI_AEVENT2_UID_ALERT_ARR_COMP_STATUS
RVA Spare Coverage | 1247 | SYMAPI_AEVENT2_UID_ALERT_DISK_SPARE_CVG
GK Utilization | 1252 | SYMAPI_AEVENT2_UID_BASED_THRESH_GK_UTIL_AVG
GK Timeout | 1253 | SYMAPI_AEVENT2_UID_BASED_GK_TIMEOUT
Storage Resource Pool Free Space | 1512 | SYMAPI_AEVENT2_UID_ALERT_FAST_SRP_ALLOC_CHANGE
Device Config Change | 1205 | SYMAPI_AEVENT2_UID_ALERT_DEV_CONFIG_CHANGE
Event Lost Alert | 2 | SYMAPI_AEVENT2_UID_EVT_EVENTS_LOST
Event Overflow Alert | 3 | SYMAPI_AEVENT2_UID_EVT_EVENTS_OVERFLOW
SRDF Alerts | 1061 | SYMAPI_AEVENT2_UID_MOD_RDF_SIM_MSG
1062 | SYMAPI_AEVENT2_UID_MOD_RDF_ERR
SRDF/A Session | 1112 | SYMAPI_AEVENT2_UID_MOD_RDFA_INACTIVE
1113 | SYMAPI_AEVENT2_UID_MOD_RDFA_ACTIVE
1123 | SYMAPI_AEVENT2_UID_MOD_SESS_DROP_NO_RDF_LNK
1130 | SYMAPI_AEVENT2_UID_MOD_SRDFA_DROP_FROM_HOST
1131 | SYMAPI_AEVENT2_UID_MOD_SRDFA_DROP_PEND_FROM_HOST
1132 | SYMAPI_AEVENT2_UID_MOD_SRDFA_DEACTIV_FROM_HOST
1133 | SYMAPI_AEVENT2_UID_MOD_SRDFA_CONS_DEACTIV_FROM_HOST
1134 | SYMAPI_AEVENT2_UID_MOD_SRDFA_DROP
1135 | SYMAPI_AEVENT2_UID_MOD_SRDFA_DROP_PEND
1158 | SYMAPI_AEVENT2_UID_MOD_SRDFA_DROP_WPL_CP
SRDF Link Status | 1064 | SYMAPI_AEVENT2_UID_MOD_RDF_LINKS_DOWN
1065 | SYMAPI_AEVENT2_UID_MOD_RDF_LINKS_UP
1080 | SYMAPI_AEVENT2_UID_MOD_RDF_1LINK_DOWN
1081 | SYMAPI_AEVENT2_UID_MOD_RDF_1LINK_UP