Jump to main content

# Detach an IP interface from a NVMe/TCP endpoint

Unisphere provides monitoring and management for Non-Volatile Memory Express (NVMe/TCP) directors, NVMe/TCP ports, NVMe/TCP endpoints, IP interfaces, and IP routes.

## Steps

1. Select a storage system running PowerMaxOS 10 (6079).
2. Select System > iSCSI+NVMe and click NVME tab to open the NVMe dashboard.
3. Click NVMe/TCP Endpoints.
4. Select an NVMe/TCP endpoint and click Detach.
5. Select an IP interface and click OK.