Jump to main content

# View embedded applications

Unisphere supports the display of embedded applications.

## Prerequisites

Embedded applications are installed on the storage system.

## About this task

See Understanding serviceability for an overview of the Unisphere for PowerMax Serviceability functionality.

## Steps

1. Select the storage system.
2. Select Serviceability > Serviceability.
   The following properties display:

   Application | The applications installed on the system.
   Version | Application version.
   Status | Application status.

   For more information about the applications details, select the application and the Applications window displays.

3. Click the NTP Server tab.
   The NTP Server IP address displays. Use this view, to view or change the NTP Server IP address.

   | NOTE: Ensure that the NTP Server IP address is reachable from the network where the Unisphere for PowerMax application is running.

4. Click the IP Configuration tab to create IPv4 and IPv6 IP addresses.
   The IPV4 view displays:
   - NAT1 IP
   - NAT Netmask
   - Nat1 Gateway
   - NAT2 IP
   - NAT2 Netmask
   - NAT2 Gateway
   IPV6 view displays Unisphere/SE-Management:
   - NAT1 IP
   - NAT1 Prefix
   - NAT1 Gateway
   - NAT2 IP
   - NAT2 Prefix
   - NAT2 Gateway