Jump to main content

# View IP routes

Unisphere provides monitoring and management for Non-Volatile Memory Express (NVMe/TCP) directors, NVMe/TCP ports, NVMe/TCP endpoints, IP interfaces, and IP routes.

## Steps

1. Select a storage system running PowerMaxOS 10 (6079).
2. Select System > iSCSI+NVMe and click NVME tab to open the NVMe dashboard.
3. Click IP Routes.
   The following properties display, depending on the operating environment:

   Destination IP | The IPv4 or IPv6 destination IP address of the IP route.
   Prefix | The IPv4 or IPv6 network mask prefix of the IP route.
   Gateway IP | The gateway IP address of the IP route.
   Network ID | The network identity of the IP route.
   Director | The director with which the IP route is associated.

   To see more information about a NVMe/TCP IP route, select it and click .

   The following parameters are displayed:
   - Destination IP —The IPv4 or IPv6 destination IP address of the IP route
   - Prefix—The IPv4 or IPv6 network mask prefix of the IP route
   - Gateway IP—The gateway IP address of the IP route
   - Network ID—The network identity of the IP route
   - Director—The director with which the IP route is associated.
   The following controls are available, depending on the operating environment:
   - Create— Create an IP route
   - —Delete an IP route