Jump to main content

# FE Port metrics

Unisphere collects and displays metrics for FE ports.

Within the PM metrics section, V4 is used to denote that the metric is supported only by a storage system (array) running PowerMaxOS 10 (6079). V3 is used to denote that the metric is supported only by a storage system (array) running HYPERMAX OS 5977 or PowerMaxOS 5978. Metrics without the denotation are supported by all storage systems (arrays).

The following table lists all metrics that are available for FE ports.

Table 1. FE port metrics
Metric | Description
--- | ---
% Busy | The percentage of time the port is busy
Avg IO Size | Calculated value: (HA Kbytes transferred per sec/total I/Os per sec)
Bad Receive Char Count | The bad receive character count - covers cases where an ordered set was received with improper encoding
Discarded Frames Count | The discarded frames count - frames can be discarded due to corruption, being out-of-order, unexpected delimiter, and so on
Expired Frames Count | The expired frames count - frames can be discarded due to a timeout occurring when waiting for something (credit, DMA engine or something protocol dependent, and so on)
Host IOs/sec | The number of I/Os the port is performing on behalf of the specific SG
Host Throughput | The number of MBs the port is processing on behalf of the specific SG
Invalid CRC Count | Invalid CRC count - covers cases where the frame received with an incorrect CRC
iSCSI Checksum Error Count | The percent of time that the port is busy
Link Failure Count | The link failure count - covers cases where the link was up but then something went wrong at the lowest level (order sets, link recovery issues, NOS, and so on)
Loss of Signal Count | The loss of signal count - covers cases where the signal was present but then was lost
Loss of Sync Count | The loss of Synchronization count - covers cases where the signal was present and timing was synced, but then sync was lost
Max Speed | Maximum potential port speed
Primitive Sequence Error Count | The primitive sequence error count - covers cases where there was a violation of low-level link management protocol (primitive sequences).
Read RT | The average time that it takes to serve one read I/O
Reads/sec | The number of read operations performed by the port per second
Received EOFA Count | The received EOFA count - covers cases where the frame was received with a particular END-OF-FRAME delimiter indicating it should be aborted or discarded.
Response Time | The average response time for the reads and writes
Rx Power | Received Power Light Level - a measurement of the strength of the signal being received by the optic
Speed | Negotiated port speed
Throughput Read | The read throughput (MBs) of the port per second
Throughput Written | The write throughput (MBs) of the port per second
Tx Power | Transmit Power Light Level - a measurement of the strength of the signal being transmitted by the optic
Write RT | The average time that it takes to serve one write I/O.
Writes/sec | The number of write operations performed each second by the port