Jump to main content

# View embedded VASA VP settings details

Unisphere supports the display of embedded applications.

## Prerequisites

Embedded applications are installed on the storage system.

## About this task

See Understanding serviceability for an overview of the Unisphere for PowerMax Serviceability functionality.

## Steps

1. Select the storage system.
2. Select Serviceability > Applications > VASA.
3. Select the VP settings tab.
   Select VASA 0 or VASA 1 from the left panel. The following properties display:
   - VP Log File Size(MB)- Select the VP Log File Size from the drop-down list. The default value is 64.
   - VP Log Level - Select error, info (default setting), debug, warning, or trace from the drop-down menu.
   - Number of Log Files to be Retained- Select the number of log files to be retained between 1 and 10. The default value is 10.
   - Maximum Concurrent Connection Per Session- Select a number between 1 and 16. The default value is 8.
   - Retain VP Certificate - Select TRUE or FALSE (default setting).
   - SYMAPI Debug Log- Select ENABLED or DISABLED (default setting).
4. Click Save to save changes, click Reset to reset the values to their defaults.

   | NOTE: The VASA application requires a reboot to apply the changes.