Jump to main content

# 1205

1205 | SYMAPI_AEVENT2_UID_ALERT_DEV_CONFIG_CHANGE
--- | ---
Category | status
Component | Device number For example: Device=1234
Severity | Info
Message | Device configuration has changed.

Unisphere policy name | Device Config Change
Action type | Alert/Refresh OM

Indicates that the configuration of some device has changed.

## Notes

- The following aspects of a device's configuration is considered by this event:
  - The base device configuration.
  - The meta configuration of the device (META_HEAD, META_MEMBER).
  - The bound-vs-bound state of a TDEV (bound vs unbound).
  - Whether a dynamic spare disk is invoked for the device.
  - The RDF mode of the device (of either leg for Concurrent SRDF).
  - The data pool bound to by a TDEV changes. This reflects a device being bound, unbound or re-bound to a different pool, and is also triggered when the name of the pool changes.