Jump to main content

# View and filter SAN health report

The SAN Health Report view allows the user to determine the health of their storage network.

## Steps

1. Select a storage system running PowerMaxOS 10 (6079).
2. Select the System Health tab.
3. In the Actions panel, click VIEW SAN HEALTH REPORT.
   The following properties display:
   - Initiator -Initiator ID
   - FCID- Fibre Channel ID for the initiator
   - Fabric WWN-Fabric WWN
   - HBA Negotiated Speed-Host bus adapter (HBA) negotiated speed
   - HBA BW Limit (Gb/Sec)-HBA bandwidth limit
   - Health Status-Health status indication - for example, a warning icon appears when port speeds of multiple director ports are greater than HBA negotiated speeds.
4. Click to view additional properties.
   The following properties display for a selected masked director port:
   - Director Identification-Director ID
   - Director Port-Port associated with the director
   - Array Negotiated Speed (Gb/Sec)-Array negotiated speed
   - Director Port Speed (Gb/Sec)-Director port speed
   The following properties display for a selected storage group:
   - Director Identification-Director ID
   - Director Port-Port associated with the director
   - Array Negotiated Speed (Gb/Sec)-Array negotiated speed
   - Director Port Speed (Gb/Sec)-Director port speed
   - Director Identification-Director ID
   - Director Port-Director port
   - Array Negotiated Speed (Gb/Sec)-Array negotiated speed
   - Director Port Speed (Gb/Sec)-Director port speed
5. You can filter the report by All Storage Groups or by All Director Ports
   For the storage group filtered report, only storage groups that are in a masking view are displayed. For the director port filtered report, only initiators and director ports that are in a masking view are displayed. The filters cannot be used together.