Jump to main content

# SRDF group SRDF/A flags

SRDF groups provide a collective data transfer path linking volumes of two separate storage systems.

Flag | Status
--- | ---
(C) Consistency | X = Enabled, . = Disabled, - = N/A
(S) Status | A = Active, I = Inactive, - = N/A
(R) RDFA Mode | S = Single-session, M = MSC, - = N/A
(M) Msc Cleanup | C = MSC Cleanup required, - = N/A
(T) Transmit Idle | X = Enabled , . = Disabled, - = N/A
(D) DSE Status | A = Active, I = Inactive, - = N/A
DSE (A) Autostart | X = Enabled, . = Disabled, - = N/A