Jump to main content

# Delete an IP interface

Unisphere provides monitoring and management for NVMe/TCP directors, NVMe/TCP ports, NVMe/TCP endpoints, IP interfaces, and IP routes.

## Prerequisites

The IP interface must be detached from the NVMe/TCP endpoint in order to delete it.

## Steps

1. Select a storage system running PowerMaxOS 10 (6079).
2. Select System > iSCSI+NVMe and click the NVME tab to open the NVMe dashboard.
3. Click IP Interfaces.
4. Select an IP interface and click .
5. Click OK.

NOTICE: This content was translated using artificial intelligence (AI). It may contain errors and is provided “as is” without any warranty of any kind. To see the original (untranslated) content, please refer to the English version. If you have questions or concerns about this content, please contact Dell at Dell.Translation.Feedback@dell.com