Jump to main content

# Enable an iSCSI endpoint

Unisphere provides monitoring and management for Internet Small Computer Systems Interface (iSCSI) directors, iSCSI ports, iSCSI endpoints, IP interfaces, and IP routes.

## Prerequisites

The enable operation does not apply for unattached iSCSI endpoints associated with storage systems running PowerMaxOS 10 (6079).

## Steps

1. Select a storage system.
2. Select System > iSCSI to open the iSCSI dashboard.
3. Click iSCSI Endpoints to open the (Attached or Unattached) iSCSI endpoints list view.
4. Select an iSCSI endpoint and click Enable.
5. Click OK.

NOTICE: This content was translated using artificial intelligence (AI). It may contain errors and is provided “as is” without any warranty of any kind. To see the original (untranslated) content, please refer to the English version. If you have questions or concerns about this content, please contact Dell at Dell.Translation.Feedback@dell.com