Jump to main content

# Discover eNAS control stations

Embedded NAS (eNAS) integrates the file-based storage capabilities of VNX arrays into storage systems.

## Prerequisites

- The storage system must be running HYPERMAX OS 5977 or PowerMaxOS 5978.

## About this task

This procedure explains how to connect to an eNAS control station for the first time.

## Steps

1. Select the storage system.
2. Select System > File.
   The File Dashboard opens.
3. If eNAS is not authenticated, click the Open Authentication dialog link.
4. Type the username and password you use to access the eNAS control station and click OK.

NOTICE: This content was translated using artificial intelligence (AI). It may contain errors and is provided “as is” without any warranty of any kind. To see the original (untranslated) content, please refer to the English version. If you have questions or concerns about this content, please contact Dell at Dell.Translation.Feedback@dell.com