Jump to main content

# 1201

Table 1. SYMAPI_AEVENT2_UID_ALERT_ARRAY_STATUS
1201 | SYMAPI_AEVENT2_UID_ALERT_ARRAY_STATUS
--- | ---
Category | status
Component | -
Severity | If Online: Normal If Online Degraded: Warning If Offline: Major If Not Present: Warning or Major (depending on situation) If Unknown: Warning or Major (depending on situation)
Message | Array state has changed to [Not Present | Unknown | Online | Write Disabled | Offline | Failed].

## Notes

- This event reflects the overall state of the array - including its Disks, Directors, Ports.
- 'Not Present' means that the array couldn't be seen by Solutions Enabler.
- 'Online' means that the array is operational.
- 'Unknown' means that:
  - One or more Ports are in an Offline or Write-Disabled state.
  - One or more Directors are in an Offline or Dead state.
  - Device events [1200] events are also enabled and one or more device is in a Not-Ready state.
  - Array subcomponent events [1204] are also enabled and one or more are in a failed (Offline) state (Fans, Power Supplies, LCCs, MIBEs, Enclosures, etc.).
- 'Failed' means that there was a problem communicating with the array.

NOTICE: This content was translated using artificial intelligence (AI). It may contain errors and is provided “as is” without any warranty of any kind. To see the original (untranslated) content, please refer to the English version. If you have questions or concerns about this content, please contact Dell at Dell.Translation.Feedback@dell.com