Jump to main content

# 5200

Table 1. SPA event
5200 | SPA event
--- | ---
Category | Event
Component | SPA
Severity | -
Message | -

Events generated by the SPA have the appropriate OID information to a given event (such as a "device configuration change"), but the Event Code (OID 1.3.6.1.4.1.1139.3.8888.2.0) displays a value of 5200 instead of the corresponding Event Code generated by the Event Daemon (for example 1205 in the case of a "device configuration change").

NOTICE: This content was translated using artificial intelligence (AI). It may contain errors and is provided “as is” without any warranty of any kind. To see the original (untranslated) content, please refer to the English version. If you have questions or concerns about this content, please contact Dell at Dell.Translation.Feedback@dell.com