Jump to main content

# Modify a serviceability VASA virtual host

Unisphere for PowerMax supports the management of serviceability VASA virtual hosts.

## Prerequisites

See Roles and associated permissions to determine the user roles that can perform this task.

## About this task

See Understanding serviceability for an overview of the Unisphere for PowerMax Serviceability functionality.

## Steps

1. Select the storage system.
2. Select Serviceability > Applications > VASA > Virtual Hosts.
3. Select a VASA system.
4. Select a virtual host.
5. Click Modify Virtual Host .
6. If you want to use IPV6 addresses in the virtual host modification, select the checkbox to indicate so.
7. Click Choose File to import a CA signed certificate file.
8. Click Modify.

NOTICE: This content was translated using artificial intelligence (AI). It may contain errors and is provided “as is” without any warranty of any kind. To see the original (untranslated) content, please refer to the English version. If you have questions or concerns about this content, please contact Dell at Dell.Translation.Feedback@dell.com