Jump to main content

# RBAC roles for SRDF local and remote replication actions

A user must be assigned the necessary roles to perform SRDF local and remote replication actions.

The following table details the roles that can perform SRDF local and remote replication actions:

| NOTE: Unisphere for PowerMax does not support RBAC device group management.

Table 1. Permissions for Local Replication, Remote Replication, and Device Management roles
Permissions | Local Replication | Remote Replication | Device Manager
--- | --- | --- | ---
SRDF Delete | No | Yes | No
SRDF Establish | No | Yes | No
SRDF Failback | No | Yes | No
SRDF Failover | No | Yes | No
SRDF Invalidate | No | Yes | No
SRDF Move | No | Yes | No
SRDF Not Ready | No | Yes | No
SRDF R1 Update | No | Yes | No
SRDF Ready | No | Yes | No
SRDF Refresh | No | Yes | No
SRDF Restore | No | Yes | No
SRDF Resume | No | Yes | No
SRDF RW Disable R2 | No | Yes | No
SRDF RW Enable | No | Yes | No
SRDF Set Bias | No | Yes | No
SRDF Set Consistency | No | Yes | No
SRDF Set Mode | No | Yes | No
SRDF Set SRDF/A | No | Yes | No
SRDF Split | No | Yes | No
SRDF Suspend | No | Yes | No
SRDF Swap | No | Yes | No
SRDF Write Disable | No | Yes | No

NOTICE: This content was translated using artificial intelligence (AI). It may contain errors and is provided “as is” without any warranty of any kind. To see the original (untranslated) content, please refer to the English version. If you have questions or concerns about this content, please contact Dell at Dell.Translation.Feedback@dell.com