Jump to main content

# 5000

Table 1. SMC event
5000 | SMC event
--- | ---
Category | Event
Component | SMC
Severity | -
Message | -

Events generated by the SMC have the appropriate OID information to a given event (such as a "device configuration change"), but the Event Code (OID 1.3.6.1.4.1.1139.3.8888.2.0) displays a value of 5000 instead of the corresponding Event Code generated by the Event Daemon (for example 1205 in the case of a "device configuration change").

NOTICE: This content was translated using artificial intelligence (AI). It may contain errors and is provided “as is” without any warranty of any kind. To see the original (untranslated) content, please refer to the English version. If you have questions or concerns about this content, please contact Dell at Dell.Translation.Feedback@dell.com