Jump to main content

# Launch Unisphere for VNX

Embedded NAS (eNAS) integrates the file-based storage capabilities of VNX arrays into storage systems.

## Prerequisites

- See Roles and associated permissions to determine the user roles that can perform this task.
- The storage system must be running HYPERMAX OS 5977 or PowerMaxOS 5978.

## Steps

1. Select the storage system.
2. Select System > File.
3. If prompted, type the username and password you use to access the eNAS control station, and click OK.
4. In the Actions panel, click Launch Unisphere for VNX.

NOTICE: This content was translated using artificial intelligence (AI). It may contain errors and is provided “as is” without any warranty of any kind. To see the original (untranslated) content, please refer to the English version. If you have questions or concerns about this content, please contact Dell at Dell.Translation.Feedback@dell.com