Jump to main content

# Host IO Limit by SG analyze view (Diagnostic and Historical)

Analyze views provide in-depth drill-down on storage system data for various collection ranges.

Table 1. Host IO Limit by SG analyze view (Diagnostic and Historical)
Attribute | Description
--- | ---
ID | The name of the storage group
Host IOs/sec | Number of I/Os the FE port is completing for the storage group
Read RT (ms) | The average time that it takes to serve one read I/O for this storage group
Write RT (ms) | The average time that it takes to serve one write I/O for this storage group
Host IO Limit IOs/sec | The number of I/Os the FE port is processing on behalf of the specific storage group
Host IO Limit Limit MBs/sec | The number of MBs the FE port is processing on behalf of the specific storage group
Host IO Limit Exceeded secs | The number of I/Os the FE port is performing on behalf of the specific storage group

NOTICE: This content was translated using artificial intelligence (AI). It may contain errors and is provided “as is” without any warranty of any kind. To see the original (untranslated) content, please refer to the English version. If you have questions or concerns about this content, please contact Dell at Dell.Translation.Feedback@dell.com