Jump to main content

# 1247

Table 1. SYMAPI_AEVENT2_UID_ALERT_DISK_SPARE_CVG
1247 | SYMAPI_AEVENT2_UID_ALERT_DISK_SPARE_CVG
--- | ---
Category | status
Component | Disk identifier, for example:
    Disk=16B:C2
(for Director 16B, DA InterfaceC, SCSI ID/Target 2)
Severity | INFO
Message | One of the following: Disk has spare coverage. Disk no longer has spare coverage.

Table 2. Unisphere policy name
Unisphere policy name | RVA Spare Coverage
--- | ---
Action type | Alert

## Note

This event is only supported on VMAX arrays running HYPERMAX OS 5977.

NOTICE: This content was translated using artificial intelligence (AI). It may contain errors and is provided “as is” without any warranty of any kind. To see the original (untranslated) content, please refer to the English version. If you have questions or concerns about this content, please contact Dell at Dell.Translation.Feedback@dell.com