Jump to main content

# Set initiator attributes

Unisphere host management includes the management of initiators and initiator groups. An initiator group is a container of one or more host initiators.

## Prerequisites

See Roles and associated permissions to determine the user roles that can perform this task.

Any changes made to the attributes of the initiator affect the initiator and all its ports.

## About this task

To set initiator attributes:

## Steps

1. Select the storage system.
2. Select Hosts > Initiators.
3. Select an initiator and click Set Attributes.
4. Type a value for the fibre channel identity (FCID) value.
5. Click OK.

NOTICE: This content was translated using artificial intelligence (AI). It may contain errors and is provided “as is” without any warranty of any kind. To see the original (untranslated) content, please refer to the English version. If you have questions or concerns about this content, please contact Dell at Dell.Translation.Feedback@dell.com