Jump to main content

# 1249

Table 1. SYMAPI_AEVENT2_UID_ALERT_SPINDLE_SPARE_CVG
1249 | SYMAPI_AEVENT2_UID_ALERT_SPINDLE_SPARE_CVG
--- | ---
Category | status
Component | Disk identifier, for example:
    Disk=16B:C2
(for Director 16B, DA InterfaceC, SCSI ID/Target 2)
Severity | Info
Message | One of the following: Disk has spare coverage. Disk no longer has spare coverage.

NOTICE: This content was translated using artificial intelligence (AI). It may contain errors and is provided “as is” without any warranty of any kind. To see the original (untranslated) content, please refer to the English version. If you have questions or concerns about this content, please contact Dell at Dell.Translation.Feedback@dell.com