Jump to main content

# RDFA Groups analyze view (Diagnostic and Historical)

SRDF groups are used to define relationships between two arrays that are logically connected using Symmetrix |Remote Data Facility (SRDF). SRDF/A groups are SRDF groups that are configured with devices running in asynchronous mode.

Table 1. RDFA Groups analyze view (Diagnostic and Historical)
Attribute | Description
--- | ---
ID | Displays the SRDF/A group number
RDFA Group Label | Displays the SRDF/A group name
RDF Response Time (ms) | SRDF response time (in milliseconds)
Duration of Last Cycle | The number of seconds for the last cycle in the session
RDF R1 to R2 MBs/sec | The throughput in MB per second from the R1 to the R2 for the SRDF/A group
RDF/A WP Count | The number of cache slots in use by the SRDF/A group
Local WP Count | The number of write pending slots waiting to be de-staged to disk - the R1 should be less than or equal to the system write pending count.
DSE Used Tracks | The number of tracks used by DSE for the SRDF/A group
% Compressed MBs Sent | The percent of total MBs sent by the director that were compressed MBs

NOTICE: This content was translated using artificial intelligence (AI). It may contain errors and is provided “as is” without any warranty of any kind. To see the original (untranslated) content, please refer to the English version. If you have questions or concerns about this content, please contact Dell at Dell.Translation.Feedback@dell.com