Jump to main content

# Set mode on a DR session within an SRDF/Metro Smart DR environment

SRDF/Metro Smart DR is a two-region high available (HA) disaster recovery (DR) solution. It integrates SRDF/Metro and SRDF/A enabling HA DR for a Metro session.

## Prerequisites

See Roles and associated permissions to determine the user roles that can perform this task.

The storage system must be running PowerMaxOS 5978 Q3 2020 or later.

## About this task

A set mode acp_disk sets the DR mode to adaptive copy disk mode. A set mode async sets the DR mode to Asynchronous mode.

To set mode on a DR session within a smart DR environment:

## Steps

1. Select the storage system.
2. Click PROTECTION to view the PROTECTION dashboard and select SRDF/MetroDR from the High Availability section of the summary panel. Alternatively, select DATA PROTECTION > MetroDR.
3. Select a smart DR environment and click DR > Set Mode.
4. Select the mode for the DR session.
5. Optional: Click Advanced Options to set the advanced options. Select the advanced options and click OK.
6. Do one of the following:
   - Click Run Now to perform the operation now.
   - Expand Run Now and click Add to Job List to add this task to the job list, from which you can schedule or run the task at your convenience. For more information, see Schedule jobs and Preview jobs.

NOTICE: This content was translated using artificial intelligence (AI). It may contain errors and is provided “as is” without any warranty of any kind. To see the original (untranslated) content, please refer to the English version. If you have questions or concerns about this content, please contact Dell at Dell.Translation.Feedback@dell.com