Jump to main content

# 1204

Table 1. SYMAPI_AEVENT2_UID_ALERT_DISK_STATUS
1204 | SYMAPI_AEVENT2_UID_ALERT_DISK_STATUS
--- | ---
Category | status
Component | Spindle ID (Disk identifier is supported for internal disks only) , for example:
    Disk=123
or
    Disk=16B:C2
(for Director 16B, DA Interface C, SCSI ID/Target 2) (internal disks only)
Severity | If Online: Normal If Online Spare: Normal If Online Degraded: Warning If Offline: Warning If Offline Spare: Warning If Not Present: Info
Message | Disk state is now <State> Where State can be: Online Offline Online Spare Offline Spare Online Degraded Not Present

Table 2. Unisphere policy name
Unisphere policy name | Disk status
--- | ---
Action type | Alert

## Notes

- 'Not Present' means that the disk could not be seen by Solutions Enabler.
- 'Online' means that one or more of the disk's Hypers are in a Ready state.
- 'Online Spare' means that the disk is a Spare and one or more of the disk's Hypers are in a Ready state.
- 'Online [Degraded]' means that the disk can only be reached via a single array DS controller. This disk state is for external disks only.
- 'Offline' means that all of the disk's Hypers are in a Not-Ready state.
- 'Offline Spare' means that the disk is a Spare and all of the disk's Hypers are in a Not-Ready state

NOTICE: This content was translated using artificial intelligence (AI). It may contain errors and is provided “as is” without any warranty of any kind. To see the original (untranslated) content, please refer to the English version. If you have questions or concerns about this content, please contact Dell at Dell.Translation.Feedback@dell.com