Jump to main content

# Host IO Limit by FE analyze view (Diagnostic and Historical)

Analyze views provide in-depth drill-down on storage system data for various collection ranges.

Table 1. Host IO Limit by FE analyze view (Diagnostic and Historical)
Attribute | Description
--- | ---
ID | The name of the director
Host IOs/sec | Number of I/Os the FE port is completing for the specific storage group
Host IO Limit IOs/sec | Number of I/Os the FE port is completing for the specific storage group
Host MBs/sec | Number of MBs per second being processed for the specific storage group
Host IO Limit MBs/sec | The Host I/O delayed I/Os divided by the I/O count
Host IO Limit Exceeded Secs | The number of I/Os the FE port is performing on behalf of the specific SG

NOTICE: This content was translated using artificial intelligence (AI). It may contain errors and is provided “as is” without any warranty of any kind. To see the original (untranslated) content, please refer to the English version. If you have questions or concerns about this content, please contact Dell at Dell.Translation.Feedback@dell.com