Jump to main content

# 1056

Table 1. SYMAPI_AEVENT2_UID_MOD_M1_RESYNC_M2
1056 | SYMAPI_AEVENT2_UID_MOD_M1_RESYNC_M2
--- | ---
Category | device
Component | Device (For example, Device=1234)
Severity | Info
Message | M1 mirror resynchronizing with its M2 mirror.

## Notes

Drive replacements/BCV activity. There is no action required because the drives are in a synchronized state.

NOTICE: This content was translated using artificial intelligence (AI). It may contain errors and is provided “as is” without any warranty of any kind. To see the original (untranslated) content, please refer to the English version. If you have questions or concerns about this content, please contact Dell at Dell.Translation.Feedback@dell.com