Jump to main content

# 1054

Table 1. SYMAPI_AEVENT2_UID_MOD_DISKDRV_SPARE_INVK
1054 | SYMAPI_AEVENT2_UID_MOD_DISKDRV_SPARE_INVK
--- | ---
Category | disk
Component | Disk [not present in logged events]
Severity | Warning
Message | Spare invoked against a disk.

Table 2. Unisphere policy
Unisphere policy name | Hotspare Invoked
--- | ---
Action type | Alert
Solutions Enabler mapping | This alert is registered as a result of registering for SYMAPI_AEVENT2_UID_ALERT_HOTSPARE_CHANGE

## Notes

The following identifies the Symmetrix errors:

- 0x0006 — Spare invoked on a failing device.
- 0x0052 — Spare invoked (mirror mask changed).

NOTICE: This content was translated using artificial intelligence (AI). It may contain errors and is provided “as is” without any warranty of any kind. To see the original (untranslated) content, please refer to the English version. If you have questions or concerns about this content, please contact Dell at Dell.Translation.Feedback@dell.com