Jump to main content

# 1248

Table 1. SYMAPI_AEVENT2_UID_ALERT_DISK_SPARE_PCT_CHNG
1248 | SYMAPI_AEVENT2_UID_ALERT_DISK_SPARE_PCT_CHNG
--- | ---
Category | status
Component | The Symmetrix Disk group number (decimal), for example:
    DiskGrp=2
Severity | INFO
Message | The spare capacity for disk group on engine [0..9]+ has changed to [0..100] percent.

## Note

This event is only supported on VMAX arrays running HYPERMAX OS 5977.

NOTICE: This content was translated using artificial intelligence (AI). It may contain errors and is provided “as is” without any warranty of any kind. To see the original (untranslated) content, please refer to the English version. If you have questions or concerns about this content, please contact Dell at Dell.Translation.Feedback@dell.com