Jump to main content

# View the NVMe dashboard

Unisphere provides monitoring and management for NVMe/TCP directors, NVMe/TCP ports, NVMe/TCP endpoints, IP interfaces, and IP routes.

## Prerequisites

The NVME tab is only enabled if there are NVMe/TCP Protocol enabled ports configured on the storage system.

## About this task

See Understanding NVMe/TCP for an overview of NVMe/TCP.

The NVMe dashboard provides you with a graphical view of the relationship between an NVMe/TCP director and its associated NVMe/TCP ports, NVMe/TCP endpoints, IP interfaces, and IP routes. From the dashboard, you can navigate to monitor and manage NVMe/TCP directors, NVMe/TCP ports, NVMe/TCP endpoints, IP interfaces, and IP routes.

To view the NVMe dashboard:

## Steps

1. Select a storage system running PowerMaxOS 10 (6079).
2. Select System > iSCSI+NVMe and click the NVME tab to open the NVMe dashboard.
   The following panels display:
   - NVMe/TCP Directors—A panel displaying the following:
     - The overall number of and relationships between the NVMe/TCP objects - NVMe/TCP Directors, unattached NVMe/TCP endpoints, attached NVMe/TCP endpoints, NVMe/TCP Ports, IP Routes, and IP Interfaces. Clicking an item opens the associated list view.
     - The list of NVMe/TCP directors - the status of the NVMe/TCP director is represented by an icon that is based on the alerts for the director. Clicking All Items results in the relationship panel displaying all NVMe/TCP Directors. Selecting a specific director results in an update to relationship panel to display director information for the selected director.
   - Actions—A panel with the following controls:
     - Create NVMe/TCP Endpoint— Create a NVMe/TCP endpoint
     - Create IP Interface— Create an IP interface
     - Create IP Route— Create an IP route
     - NVMe/TCP Configuration— Configure NVMe/TCP using a wizard
   - NVMe/TCP Alerts—A panel is displayed listing the latest alerts, the associated object, description, and creation date/time. Click View All to view all alerts. The following properties display:

     State | The state of the alert
     Severity | The severity of the alert
     Type | The alert type
     Description | The description of the alert
     Created | Date/time that the alert was created.
     Acknowledged | The date and time that the alert was acknowledged.

NOTICE: This content was translated using artificial intelligence (AI). It may contain errors and is provided “as is” without any warranty of any kind. To see the original (untranslated) content, please refer to the English version. If you have questions or concerns about this content, please contact Dell at Dell.Translation.Feedback@dell.com