Jump to main content

# View EDS directors

Unisphere supports the display of director information.

## Prerequisites

Enginuity Data Services (EDS) directors are only supported on storage systems running HYPERMAX OS 5977 or PowerMaxOS 5978.

## Steps

1. Select the storage system.
2. In the Dashboard, click the System Health tab.
3. In the Actions panel, click Other Hardware and then click the EDS tab to open the EDS list view.

   The following properties display:

   | NOTE: Some of the following properties are environment-specific and therefore may appear in a different order or not at all.

   Director | Director name.
   % Busy | Percent of time the director is busy. This field only displays when the storage system is registered with the Performance component.
   Director Type | Director type.
   Director Status | Director status.
   Cores | Number of available director cores.
   Associated Ports | Number of associated ports.
   Alerts | Director alert status, as indicated by icon color: One or more fatal alerts One or more critical alerts, with none higher One or more warning alerts, with none higher One or more informational alerts, with none higher No alerts

NOTICE: This content was translated using artificial intelligence (AI). It may contain errors and is provided “as is” without any warranty of any kind. To see the original (untranslated) content, please refer to the English version. If you have questions or concerns about this content, please contact Dell at Dell.Translation.Feedback@dell.com