Jump to main content

# Disassociate directors and ports

Unisphere supports the disassociation of directors and ports.

## Prerequisites

The storage system must be running HYPERMAX OS 5977 or PowerMaxOS 5978.

## Steps

To disassociate ports with directors:

1. Select the storage system.
2. Select System > Hardware.
3. Click the tab for the appropriate director emulation type to open its list view.
4. Select the director.
5. Click Disassociate.
6. Click OK.

NOTICE: This content was translated using artificial intelligence (AI). It may contain errors and is provided “as is” without any warranty of any kind. To see the original (untranslated) content, please refer to the English version. If you have questions or concerns about this content, please contact Dell at Dell.Translation.Feedback@dell.com