Jump to main content

# Manage file masking views

Embedded NAS (eNAS) integrates the file-based storage capabilities of VNX arrays into storage systems.

## Prerequisites

- See Roles and associated permissions to determine the user roles that can perform this task.
- The storage system must be running HYPERMAX OS 5977 or PowerMaxOS 5978.

## About this task

This procedure explains how to manage file masking views.

## Steps

1. Select the storage system.
2. Select System > File.
   The File Dashboard opens.
3. In the Summary panel, click File Masking Views.
4. Select one or more masking views and click one of the following, depending on the operation you want to perform:
   - View Path Details— View masking view connections
   - Delete— Delete masking views