Jump to main content

# 1204

Table 1. SYMAPI_AEVENT2_UID_ALERT_DISK_STATUS
1204 | SYMAPI_AEVENT2_UID_ALERT_DISK_STATUS
--- | ---
Category | status
Component | Spindle ID (Disk identifier is supported for internal disks only) , for example:
    Disk=123
or
    Disk=16B:C2
(for Director 16B, DA Interface C, SCSI ID/Target 2) (internal disks only)
Severity | If Online: Normal If Online Spare: Normal If Online Degraded: Warning If Offline: Warning If Offline Spare: Warning If Not Present: Info
Message | Disk state is now <State> Where State can be: Online Offline Online Spare Offline Spare Online Degraded Not Present

Table 2. Unisphere policy name
Unisphere policy name | Disk status
--- | ---
Action type | Alert

## Notes

- 'Not Present' means that the disk could not be seen by Solutions Enabler.
- 'Online' means that one or more of the disk's Hypers are in a Ready state.
- 'Online Spare' means that the disk is a Spare and one or more of the disk's Hypers are in a Ready state.
- 'Online [Degraded]' means that the disk can only be reached via a single array DS controller. This disk state is for external disks only.
- 'Offline' means that all of the disk's Hypers are in a Not-Ready state.
- 'Offline Spare' means that the disk is a Spare and all of the disk's Hypers are in a Not-Ready state