Jump to main content

# View embedded Solutions Enabler system details

Unisphere supports the display of embedded applications.

## Prerequisites

Embedded applications are installed on the storage system.

## About this task

See Understanding serviceability for an overview of the Unisphere for PowerMax Serviceability functionality.

## Steps

1. Select the storage system.
2. Select Serviceability > Applications > SE-MANAGEMENT.
3. Select the SYSTEM tab.
   The following properties display:
   - Access ID—Access ID
   - Application—The selected application name
   - Node Name—The node where it is installed.
   - Status—The application status
4. Click Configure Certificates.
   The Configure Certificates window displays. Select the certificate type from the drop-down menu. The following options display:

   Self-Signed Certificate | Select Replace with Self-Signed Certificate from the drop-down menu. A message displays stating This operation will replace existing certificates. Solutions Enabler must be restarted for new certificates to take effect. Select Restart Solutions Enabler. A window confirms that a daemon restart is required, select Proceed. Select Apply to create a Self-Signed Certicate. A window confirms that the action was successful. Click OK.
   Custom Certificate Upload | Select Custom Certificate Upload from the drop-down menu. A window confirms that a daemon restart is required, select Proceed. Select Choose File for one of the following: Import Alternate Key File Import Alternate Certificate Import Alternate Trust Certificate Click Restart Solutions Enabler.

5. Select the checkbox that is associated with SE-MGMT-0 or SE-MGMT-1 checkbox and then select Download Logs. Optionally select the Only local system logs checkbox.