Jump to main content

# 1217

Table 1. SYMAPI_AEVENT2_UID_DFR_SVC_STATE
1217 | SYMAPI_AEVENT2_UID_DFR_SVC_STATE
--- | ---
Category | status
Component | -
Severity | If the replacement threshold has been exceeded : Warning, Otherwise: Info
Message | The deferred services replacement threshold has been exceeded - service is required. The deferred services replacement threshold is no longer exceeded.

Table 2. Unisphere policy name
Unisphere policy name | Deferred Service Threshold Alert
--- | ---
Action type | Alert

Indicates that the Deferred Service replacement threshold indicator for a storage array has changed. This change can be in either direction - from not-exceeded to exceeded ... or from exceeded to not-exceeded.

## Note

- This event will only be generated if Deferred Service is enabled for the storage array.