Jump to main content

# Host IO Limit by FE analyze view (Diagnostic and Historical)

Analyze views provide in-depth drill-down on storage system data for various collection ranges.

Table 1. Host IO Limit by FE analyze view (Diagnostic and Historical)
Attribute | Description
--- | ---
ID | The name of the director
Host IOs/sec | Number of I/Os the FE port is completing for the specific storage group
Host IO Limit IOs/sec | Number of I/Os the FE port is completing for the specific storage group
Host MBs/sec | Number of MBs per second being processed for the specific storage group
Host IO Limit MBs/sec | The Host I/O delayed I/Os divided by the I/O count
Host IO Limit Exceeded Secs | The number of I/Os the FE port is performing on behalf of the specific SG