Jump to main content

# 1054

Table 1. SYMAPI_AEVENT2_UID_MOD_DISKDRV_SPARE_INVK
1054 | SYMAPI_AEVENT2_UID_MOD_DISKDRV_SPARE_INVK
--- | ---
Category | disk
Component | Disk [not present in logged events]
Severity | Warning
Message | Spare invoked against a disk.

Table 2. Unisphere policy
Unisphere policy name | Hotspare Invoked
--- | ---
Action type | Alert
Solutions Enabler mapping | This alert is registered as a result of registering for SYMAPI_AEVENT2_UID_ALERT_HOTSPARE_CHANGE

## Notes

The following identifies the Symmetrix errors:

- 0x0006 — Spare invoked on a failing device.
- 0x0052 — Spare invoked (mirror mask changed).