Jump to main content

# View host initiators

Unisphere host management includes the management of initiators and initiator groups. An initiator group is a container of one or more host initiators.

## Steps

1. Select the storage system.
2. Select Hosts > Hosts.
3. Select the host and click to open the host details view, and then click the link in the Initiators field to open the initiators list view.

   The following properties display:

   Initiator—WWN or IQN (iSCSI Qualified Name) ID of the initiator.

   Dir:Port—Storage system director and port that is associated with the initiator, for example: FA-7E:1.

   Alias—User-defined initiator name.

   Logged In—Flag indicating if the initiator is logged into the fabric: Yes/No.

   On Fabric—Flag indicating if the initiator is on the fabric: Yes/No.

   Port Flag Overrides—Flag indicating if any port flags have been overridden by the initiator: Yes/No.

   Hosts—Number of hosts the initiator is associated with.

   Masking Views—Number of associated masking views.

   The following controls are available:

   Set Attributes— Set initiator attributes

   Set Host Flags— Set initiator port flags

   Rename Alias— Rename initiator aliases

   Replace Initiator— Replace initiators

   Remove Masking Entry— Remove initiator from login history