Jump to main content

# View iSCSI endpoints list

Unisphere provides monitoring and management for Internet Small Computer Systems Interface (iSCSI) directors, iSCSI ports, iSCSI endpoints, IP interfaces, and IP routes.

## Steps

1. Select a storage system.
2. Select System > iSCSI to open the iSCSI dashboard.
3. Click iSCSI Endpoints (Attached or Unattached) to open the iSCSI endpoints list view and select a specific director to filter the list.
   The following properties display, depending on the operating environment:

   Name | The IQN of the iSCSI endpoint.
   Dir:Virtual Port | The assigned virtual port for the iSCSI endpoint.
   Status | The status of the iSCSI endpoint.
   Network ID | The network identity of the IP interface that provides isolated IP routes.
   IP Interfaces | The total number of IP interfaces attached to the iSCSI endpoint.
   iSCSI Ports | The total number of physical IP ports associated with the iSCSI endpoint.
   Volumes | The total number of volumes that are mapped to the iSCSI endpoint.

   The following controls are available, depending on the operating environment:
   - —View iSCSI endpoint details
   - Create— Create an iSCSI endpoint
   - Enable— Enable an iSCSI endpoint (does not apply for unattached iSCSI endpoints associated with storage systems running PowerMaxOS 10 (6079))
   - Disable— Disable an iSCSI endpoint (does not apply for unattached iSCSI endpoints associated with storage systems running PowerMaxOS 10 (6079))
   - Set Port Flags— Set port flags
   - Attach— Attach an IP interface to an iSCSI endpoint
   - Modify— Modify an iSCSI endpoint
   - Detach— Detach an IP interface from an iSCSI endpoint
   - Delete— Delete an iSCSI endpoint