Jump to main content

# View file import details

Network-attached storage is a file-level storage architecture that makes stored data more accessible to networked devices.

## Prerequisites

See Roles and associated permissions to determine the user roles that can perform this task.

## About this task

See Understanding PowerMax File for storage systems for an overview of PowerMax File.

## Steps

1. Select a storage system that supports PowerMax File migration.
2. Select Data Protection > File Migration.
3. Select File Imports.
4. Click a session name.
   The following properties display within tabs:

   DETAILS tab

   The following properties display:

   - Session Name—Name of replication session
   - Type—Session type
   - Import State—Status of the import, for example, Initialized, Ready_to_Cutover, Canceled, Error, Completed
   - Current Operation—Status of the current operation, for example, Initialized, Initial_Provisioning, Ready_to_Cutover, Canceled, Completed
   - Source NAS Server Name—Source NAS server name
   - Target NAS Server Name—Target NAS server name
   - Primary Node—Model of the remote system
   - Backup Node—Version of the remote system
   - Current Operation Progress Percentage—Percentage progress of the current operation
   - Alerts—Number of associated alerts

   NAS SERVER tab

   The following properties display:

   - Source NAS Server Name—Source NAS server name
   - Target NAS Server Name—Target NAS server name
   - Protocol Type—Protocol type, for example, SMB

   FILE SYSTEMS tab

   The following properties display:

   - Source Name —Source name
   - Source Size—Source size
   - Target Name —Target name
   - Target Size—Target size
   - State —State, for example, Idle
   - FLR Enabled—FLR enabled indication

   NETWORK INTERFACE tab

   The following properties display:

   - Source Interface Name —Source interface name
   - Target Interface Name —Target interface name
   - Netmask—Netmask
   - Prefix Length—Prefix Length
   - Gateway—Gateway IP address
   - VLAN ID—VLAN ID

   FILE IMPORT INTERFACE tab

   The following properties display:

   - IP Address—IP address
   - Gateway—Gateway IP address
   - Netmask—Netmask
   - Prefix Length—Prefix Length
   - VLAN ID—VLAN ID