Jump to main content

# File System Details

Embedded NAS (eNAS) integrates the file-based storage capabilities of VNX arrays into storage systems running HYPERMAX OS 5977 or PowerMaxOS 5978. With this integrated storage solution, storage can be provisioned to eNAS data movers, which trigger the creation of storage pools in VNX. The users of Unisphere for VNX use the storage pools for file-level provisioning, for example, creating file systems, file shares.

The File System Details view displays the following properties.

- File System Name—Name of the file system
- File System Unique ID—Unique VNX ID for the file system
- File System Total Capacity (GB)—Size of the file system
- File System Free Capacity (GB)—Available space on the file system
- File System Block Size (Bytes)—Size of a block on the file system
- File System Type—Type of file system and its conventions, for example, NTFS
- Operational Status—Current operational status of the local file system
- Storage Groups—Storage groups on the file system
- Storage Pool—Storage pools on the file system