Jump to main content

# 1247

Table 1. SYMAPI_AEVENT2_UID_ALERT_DISK_SPARE_CVG
1247 | SYMAPI_AEVENT2_UID_ALERT_DISK_SPARE_CVG
--- | ---
Category | status
Component | Disk identifier, for example:
    Disk=16B:C2
(for Director 16B, DA InterfaceC, SCSI ID/Target 2)
Severity | INFO
Message | One of the following: Disk has spare coverage. Disk no longer has spare coverage.

Table 2. Unisphere policy name
Unisphere policy name | RVA Spare Coverage
--- | ---
Action type | Alert

## Note

This event is only supported on VMAX arrays running HYPERMAX OS 5977.