Jump to main content

# 1247

1247 | SYMAPI_AEVENT2_UID_ALERT_DISK_SPARE_CVG
--- | ---
Category | status
Component | Disk identifier For example: Disk=16B:C2 (for Director 16B, DA InterfaceC, SCSI ID/Target 2)
Severity | INFO
Message | Disk has spare coverage. or Disk no longer has spare coverage.

Unisphere policy name | RVA Spare Coverage
Action type | Alert

## Note

This event is only supported on VMAX arrays running HYPERMAX OS 5977.