Jump to main content

# Understanding workload monitoring, planning, and provisioning

Unisphere supports applications that support the monitoring, planning, and provisioning of workloads.

If you have an array that is monitored for performance by Unisphere for PowerMax for at least 2 weeks you will have enough data to do a characterization of the workload for an existing storage group or multiple storage groups.

The workload planner (WLP) application performs performance impact checks (the terms performance impacts checks, admissibility checks, and suitability checks are used interchangeably) when provisioning via the Unisphere UI wizards; it performs the checks to make sure there is sufficient performance headroom before creating new application workloads on storage arrays. WLP keeps its own database which is a subset of Key Performance Indicator (KPI) metrics gathered by Unisphere for PowerMax and uses this to help make decisions, so to use it the arrays in question must be registered for performance data collection.

WLP models the internal load balancing of the array when adding additional load to an existing array. WLP can assist in placing workloads on the most suitable target array for new provisioning and/or migrated workloads. WLP can help in port group creation or selection, based on existing zoning and utilization while balancing across directors.

A Note on Data Processing and Organization

Many applications (and as a result, storage systems) experience fluctuations in workloads over time. Often, these fluctuations repeat in a predictable way. To keep the Workload Planner data footprint as small as possible, but still adequately represent the history and fluctuations in workloads, multiple weeks of historical storage system performance data are weighted and averaged into a week's worth of four-hour time windows which create a "representative workload" for all system components and applications that are applied to a storage system.

When accounting for maximum performance capabilities of a system component, best practice limits are applied. All performance impact scores and utilizations that are calculated and reported by Workload Planner are done so against these best practice Limits, not the actual maximum performance capacity of the pertinent component or components. Recommendations and performance impact scores are intentionally conservative to ensure maximum system performance is maintained.

Also, all utilizations and performance impact scores are derived from the four-hour windows. When a single value is returned, the value return is the value of the most performance limiting four-hour window value for the most limiting component on the storage system. For example, during new provisioning, the impact of adding a new workload to a front-end port could take the utilization of that port from ~30% utilized to ~35% for most time windows, but 32% to 37% on Tuesdays between 8AM and 12PM UTC. In this case, the new port utilization would be reported as 37% because that is the most limiting four-hour window value.

The four-hour window implementation allows Workload Planner to pack workloads more efficiently and realistically onto storage systems with respect to inverse performance fluctuations. For example, a workload that is heavy on weekends, but light during weekdays performs better with a second workload that is light on weekends and heavy on weekdays than a workload that is distributed similarly to itself.

One drawback to the four-hour window implementation is that it is sensitive to peaks in data. If unexpected performance impact, system headroom, and/or service level compliance results are observed, see Manage System Data Exclusion Windows for help on remediating these issues.

The following workload monitoring, planning, and provisioning tasks can be performed from Unisphere for PowerMax:

- Monitor Storage Group compliance against its service level and workload type:
  - Create service level compliance alert policies—Create service level compliance alert policies.
  - View storage group compliance—View overall Storage Group Compliance dashboard.
  - View compliance report—View compliance reports.
  - Create compliance report—Create Compliance Reports.
  - Exclude data (Manage System Data Exclusion Windows and Manage System Data Exclusion Windows).
- Perform provisioning—Provision storage.
- Perform multi array provisioning—The multi-array Provision Storage wizard.
- Perform multi array provisioning using templates—The multi-array Provision Storage wizard.
- Perform migration—Create a migration session.
- Perform multi array migration—The multi-array Migration wizard.