Jump to main content

# 1201

1201 | SYMAPI_AEVENT2_UID_ALERT_ARRAY_STATUS
--- | ---
Category | status
Component |
Severity | If Online: Normal If Online Degraded: Warning If Offline: Major If Not Present: Warning or Major (depending on situation) If Unknown: Warning or Major (depending on situation)
Message | Array state has changed to [Not Present | Unknown | Online | Write Disabled | Offline | Failed].

## Notes

- This event reflects the overall state of the array - including its Disks, Directors, Ports.
- 'Not Present' means that the array couldn't be seen by Solutions Enabler.
- 'Online' means that the array is operational.
- 'Unknown' means that:
  - One or more Ports are in an Offline or Write-Disabled state.
  - One or more Directors are in an Offline or Dead state.
  - Device events [1200] events are also enabled and one or more device is in a Not-Ready state.
  - Array sub-component events [1404] are also enabled and one or more are in a failed (Offline) state (Fans, Power Supplies, LCCs, MIBEs, Enclosures, etc.).
- 'Failed' means that there was a problem communicating with the array.